Exp 6 LED Blinking

#include<reg51.h>

char arr[10]={0x40,0x79,0x24,0x30,0x19,0x12,0x02,0x78,0x00,0x10};

void delay(void); void main(void)

{

int count; for(count=0;count<10;count++)

{

P0=arr[count]; delay();

}

}

void delay(void){

unsigned int i; for(i=0;i<1;i++);

}





